**C7042 Scalextric Digital 6 Car Advanced Powerbase Aux to USB Cable 9-Mar-2012**

This cable is an RS485 Aux RJ11 to USB converter. This is different from the cable that is used on the old 6 Car Powerbase C7030, which is 5V level RS232.



Cable is suitable for connection to the Race Management Programs and for reprogramming the firmware in the C7042 Powerbase.

A VCP Driver from FTDI is required for the PC

Aux to USB lead, based on the FTDI chip, drivers available for all operating systems.

<http://www.ftdichip.com/Drivers/VCP.htm>

Here is a link to the Installation Guides.

<http://www.ftdichip.com/Documents/InstallGuides.htm>

For Race Management, Firmware Downloads & the firmware Download Program see.

<http://ssdc.jackaments.com/>

Alternative Race Management from

<http://pclapcounter.be/>

**Note.Cables have protection diodes fitted** however the RS448 Interface chip can be damaged by unplugging at the Powerbase end when the Powerbase is powered up. **Always Plug & Unplug with Power removed from the Powerbase.**

Ordering

Price is £23.00 GBP for a 1 Meter lead..

For 2 Meters £23.50 GBP

For 3 Meters £24.00 GBP

For 4 Meters £24.50 GBP

For 5 Meters £25.00 GBP

.Longer lead lengths are possible, please add 50P / Meter.

Postage to the UK First Class add £1.00 GBP

Postage to rest of World, Air Mail, add £2.00 GBP

Payment by PayPal to richard@girling.net

Please include name & address.

**When ordering please specify cable length & that you require a lead for C7042**

If available please select the **Personal payment owed** tab as this saves the Paypal fee.

*Your address is not included automatically with a Personal Payment, please add it in the text*.